This program configures the temperature sensor on the NUCLEO-STM32F411RE to read the CPU temperature and display it with UART.

The output is the program is shown below:

|  |
| --- |
|  |

When a finger is played on the MCU’s CPU, the temperature increases slightly, as shown below:

|  |
| --- |
|  |