This program configures the NUCLEO-STM32F411RE DMA driver, sends a background message with the DMA, and displays it on the screen using the UART. Each time the reset button is pressed, the message is displayed as shown below:

|  |
| --- |
|  |