This program configures the timer interrupt and flashes the LED on PA5 on the NUCLEO-STM32F411RE at 1hz while simultaneously displaying the result on the screen using the UART.

The result is shown below:

|  |
| --- |
|  |